PRAKTIKUM III
PARTISI HARDDISK

I.	TUJUAN PRAKTIKUM

1.	Membuat partisi harddisk.
2.	Mengaktifkan partisi harddisk.
3.	Melihat informasi partisi harddisk.
4.	Menghapus partisi harddisk.

II.	PERSIAPAN

1.	Masukan CD bootable kedalam optical drive. Pastikan didalamnya mengandung file FDISK.EXE.
2.	Hidupkan computer.
3.	Masuklah ke setup BIOS. Tekanlah tombol Del berulang kali pada saat booting. Muncul menu utama setup BIOS. Pilihlah BIOS FITURE SETUP. Buatlah boot sequence menjadi “CDROM, C, A’. Keluarlah dari setup BIOS. Lakukan penyimpanan (save) pada save & exit setup. Komputer kembali melakukan booting.
4.	Tunggulah beberapa saat hingga muncul tampilan “A:\>” dilayar monitor.
5.	Ketiklah FDISK, lalu tekan ENTER.

III.	TUTORIAL PARTISI HARDDISK

MEMBUAT PARTISI

1.	SATU PARTISI

Microsoft Windows 98
Fixed Disk Setup Program
© Copyright Microsoft Corp 1983-1988

FDISK Option

Current fixed disk drive : 1

Chose one of the following:
1.	Create DOS partition or Logical DOS Drive
2.	Set active paertition
3.	Delete partition or Logical DOS Drive
4.	Display partition information

Enter choice: [1]

Press Esc to exit FDISK	

Create DOS Partition or Logical DOS Drive

Current fixed disk drive : 1

Chose one of the following:
1.	Create Primary DOS Partition
2.	Create Extended DOS Partition
3.	Create Logical DOS Drive(s) in the Extended DOS Partition
4.	Display partition information

Enter choice: [1]

Press Esc return to FDISK Options

Create DOS Partition

Current fixed disk drive: 1

Do you wish to use the maximum available size for a Primary DOS
Partition and make the partition active (Y/N) ……? [Y]

Press Esc to return to FDISK Options.	

You MUST restart your system for your changes to take effect.
Any drives you have created or changed must be formatted
AFTER you restart

Show down Windows before restarting.

Press Esc to return to FDISK Options	

2.	DUA PARTISI

A.	Partisi Primari

Microsoft Windows 98
Fixed Disk Setup Program
© Copyright Microsoft Corp 1983-1988

FDISK Option

Current fixed disk drive : 1

Chose one of the following:
1.	Create DOS partition or Logical DOS Drive
2.	Set active paertition
3.	Delete partition or Logical DOS Drive
4.	Display partition information

Enter choice: [1]

Press Esc to exit FDISK

Create DOS Partition

Current fixed disk drive: 1

Do you wish to use the maximum available size for a Primary DOS
Partition and make the partition active (Y/N) ……? [N]

Press Esc to return to FDISK Options.

Create Primary DOS Partition

Current fixed disk drive : 1

Total disk space is 810 Mbytes (1 Mbytes = 1048576)
Maximum space available partition is 810 Mbytes (100%)

Enter partition size in Mbytes or percent of disk space (%) to create a
Primary DOS Partition ……… : [500]

Press Esc to return to FDISK Options.	

Create Primary DOS Partition

Current fixed disk drive : 1

Partition	Status	Type	Volume Label	Mbytes	System		Usage
C:1			PRI DOS		500		UNKNOWN	62%	

Primary DOS Partition created

Press Esc to return to FDISK Options.

B.	Partisi Extended

Microsoft Windows 98
Fixed Disk Setup Program
© Copyright Microsoft Corp 1983-1988

FDISK Option

Current fixed disk drive : 1

Chose one of the following:
1.	Create DOS partition or Logical DOS Drive
2.	Set active paertition
3.	Delete partition or Logical DOS Drive
4.	Display partition information

Enter choice: [1]

Press Esc to exit FDISK

Create DOS Partition or Logical DOS Drive

Current fixed disk drive : 1

Chose one of the following:
1.	Create Primary DOS Partition
2.	Create Extended DOS Partition
3.	Create Logical DOS Drive(s) in the Extended DOS Partition
4.	Display partition information

Enter choice: [2]

Press Esc return to FDISK Options

Create Extended DOS Partition

Current fixed disk drive : 1

Total disk space is 810 Mbytes (1 Mbytes = 1048576)
Maximum space available partition is 310 Mbytes (38%)

Enter partition size in Mbytes or percent of disk space (%) to create an
Extended DOS Partition ……… : [310]

Press Esc to return to FDISK Options.

Create Logical DOS Partition

No logical drives defind

Total Extended DOS Partition size is 310 Mbytes (1 Mbytes = 1048576bytes)
Maximum space available for logical drive is 310 Mbytes (100%)

Enter logical drive size in Mbytes or percent of disk space (%) ………[310]

Press Esc to return to FDISK Options.	

You MUST restart your system for your changes to take effect.
Any drives you have created or changed must be formatted
AFTER you restart

Show down Windows before restarting.

Press Esc to return to FDISK Options

MENGAKTIFKAN PARTISI

Microsoft Windows 98
Fixed Disk Setup Program
© Copyright Microsoft Corp 1983-1988

FDISK Option

Current fixed disk drive : 1

Chose one of the following:
1.	Create DOS partition or Logical DOS Drive
2.	Set active paertition
3.	Delete partition or Logical DOS Drive
4.	Display partition information

Enter choice: [2]

Press Esc to exit FDISK	

Set Active Partition

Current fixed disk drive : 1

Partition	Status	Type	Volume Label	Mbytes	System		Usage
C:1		A	PRI DOS		500		FAT16		62%
    2			EXTDOS		310				38%

Total disk space is 810 Mbytes (1 Mbytes = 1048576 bytes)
Enter the number of the partition you want to make active ………………….[1]

Press Esc to return to FDISK Options.

MENAMPILKAN PARTISI

Microsoft Windows 98
Fixed Disk Setup Program
© Copyright Microsoft Corp 1983-1988

FDISK Option

Current fixed disk drive : 1

Chose one of the following:
1.	Create DOS partition or Logical DOS Drive
2.	Set active paertition
3.	Delete partition or Logical DOS Drive
4.	Display partition information

Enter choice: [4]

Press Esc to exit FDISK	

Display Partition Information

Partition	Status	Type	Volume Label	Mbytes	System		Usage
C:1		A	PRI DOS		500		FAT16		62%
    2			EXTDOS		310				38%

Total disk space is 810 Mbytes (1 Mbytes = 1048576 bytes)

The Extended DOS Partition contains Logical DOS Drive
Do you want to display the logical drive information [Y/N] ……………….?[Y]

Press Esc to return to FDISK Options.

Display Logical DOS drive information

Drv	Volume Label		Mbytes	System		Usage
D				310		FAT16		100%

Total Extended DOS Partition size is 310 Mbytes (1 Mbytes = 1048576 bytes)

Press Esc to return to FDISK Options.

MENGHAPUS PARTISI

1.	PARTISI PRIMARI

Microsoft Windows 98
Fixed Disk Setup Program
© Copyright Microsoft Corp 1983-1988

FDISK Option

Current fixed disk drive : 1

Chose one of the following:
1.	Create DOS partition or Logical DOS Drive
2.	Set active paertition
3.	Delete partition or Logical DOS Drive
4.	Display partition information

Enter choice: [3]

Press Esc to exit FDISK
	
Delete Partition or Logical DOS Drive

Current fixed disk drive : 1

Choose one of the following :
1.	Delete Primary DOS Partition
2.	Delete Extended DOS Partition
3.	Delete Logical DOS Drive (s) in the Extended DOS Partition
4.	Delete Non-DOS Partition

Enter choice : [1]

Press Esc to return to FDISK Option	

Delete Primary DOS Partition

Partition	Status	Type	Volume Label		Mbytes	System		Usage
C:1		A	PRI DOS			500		FAT16		62%

Total disk space is 810 Mbytes (1 Mbytes = 1048576 bytes)

WARNING ! Data in the deleted Extended DOS partition will be lost
What Primary partition do you want to delete ………………………...? [1]
Enter volume label …………………………………………………….? [ ………]
Are you sure (Y/N) ……………………………………………………? [Y]

Press Esc to return to FDISK Option

2.	PARTISI LOGICAL

Microsoft Windows 98
Fixed Disk Setup Program
© Copyright Microsoft Corp 1983-1988

FDISK Option

Current fixed disk drive : 1

Chose one of the following:
1.	Create DOS partition or Logical DOS Drive
2.	Set active paertition
3.	Delete partition or Logical DOS Drive
4.	Display partition information

Enter choice: [3]

Press Esc to exit FDISK

Delete Partition or Logical DOS Drive

Current fixed disk drive : 1

Choose one of the following :
1.	Delete Primary DOS Partition
2.	Delete Extended DOS Partition
3.	Delete Logical DOS Drive (s) in the Extended DOS Partition
4.	Delete Non-DOS Partition

Enter choice : [3]

Press Esc to return to FDISK Option

Delete Logical DOS Drive (s) in the Extended DOS Partition

Partition	Status	Type	Volume Label		Mbytes	System		Usage
D:							310		FAT16		100%

Total disk space is 310 Mbytes (1 Mbytes = 1048576 bytes)

WARNING ! Data in the deleted Logical DOS Drive will be lost
What drive do you want to delete ……………………………………...? [D]
Enter volume label …………………………………………………….? [ ………]
Are you sure (Y/N) ……………………………………………………? [Y]

Press Esc to return to FDISK Option

Delete Extended DOS Partition

Partition	Status	Type	Volume Label		Mbytes	System		Usage
C:1		A	PRI DOS			510		FAT16		62%
    2			EXT DOS			310				38%

Total disk space is 310 Mbytes (1 Mbytes = 1048576 bytes)

WARNING ! Data in the deleted Logical DOS Drive will be lost
Do you wish to continue (Y/N) …………………………………..? [Y]

Press Esc to return to FDISK Option

IV.	TUGAS PRAKTIKUM

1.	Jelaskan sejauh mana peranan dan fungsi setup BIOS dalam instalasi komputer.
2.	Menurut Anda apakah perlu melakukan setup BIOS ? Dan kapan Anda harus melakukan setup BIOS ?
3.	Menurut Anda, apakah setiap kita menambahkan perangkat yang baru atau mengganti perangkat yang rusak dengan yang baru harus melakukan setup BIOS terlebih dahulu atau tidak ? Jelaskan alasan Anda ?
4.	Jelaskan sejauh mana peranan power option dalam control panel ?
5.	Menurut Anda apa fungsi dan keutamaan dari device manager ?
6.	Untuk hal apakah tujuan dan fungsi dari dxdiag ?
7.	Kenapa pada windows XP sering muncul tampilan blue screen ?
8.	Dan apakah itu blue screen ?